Practical-3

**AIM:** Allocating IP address to network topologies

Student should be able to apply IP addresses to

1. Topology: two directly connected computers
2. Topology: four computers connected by switches
3. Topology: two networks connected by Router Various networking commands:

* ping
* ipconfig
* arp –a
* netstat
* netbios
* tracert
* hostname
* nmap Reference Videos

1. Refer Video(25 minutes) of practical-4
2. IP address: <https://www.youtube.com/watch?v=ykz4oUPWACw>
3. IP address assignment in Video: <https://www.youtube.com/watch?v=vcAtxgDsl00> Reference for commands:
4. <https://lizardsystems.com/articles/network-command-line-utilities/>
5. <https://www.youtube.com/watch?v=nH85pddWWAk>
6. <https://www.youtube.com/watch?v=rurs7cdT5cc&t=7s>

**Note:** While applying IP address, student needs to allocate IP address as per his/her student ID. For Example, if student ID is 20ce005 then IP address allocation for the first network should start with 5.0.0.0. For subsequent networks, it should start with ID+1 i.e. 6.0.0.0, 7.0.0.0 and so on.


**Submission**: After writing an answer into this word document, Student needs to change name to his ID followed by practical number. Ex 20ce005\_Pr1.docx. Upload on assignment segment.

**Rubrics**: Nicely drafted document with clarity in answers leads to full marks. Otherwise, submission carries proportional marks.

**Recommended** to type, avoid copy-paste to increase your typing skill.

# Refer to the following scenarios and let’s understand What is an IP Address

**and Purpose of IP Address. Scenario : 1**



In this first scenario, an envelope is sent from sachana to kathlal. But there was some check point like ahmedabad, kathwada and then the envelope is delivered to kathlal.

Justify the following statement.

1. Was there any difficulty faced during sending the envelope from sender to receiver ?

# Scenario : 2




In this second scenario, the sender was located at Ahmedabad and wanted to send a file to the receiver who was located at Gandhinagar. But at the time of sending a file to the receiver, the receiver's machine was powered off. So, can the receiver receive the file from the sender or not?

Justify the following statement.

1. Was there any difficulty faced during sending the file from sender to receiver? If yes then what would be the solution for it.


# Scenario: 3



Refer the above image, and justify your answer Question:

Can the envelope be sent to the proper destination?

# Scenario: 4



An IP address also acts like a return address on postal mail. When a letter you've mailed is delivered to the wrong address, you get the letter back if you include a return address on the envelope. The same holds true for email. When you write to an invalid recipient (such as someone who left their job and no longer has a company email address) your IP address lets the company’s mail server send you back a bounce message so that you know your email wasn't sent to the right place.

# From the above all scenarios, what would be the conclusion? IP Address Types


Basically, there are two primary types of ip address formats used today.

## IPv4

1. **IPv6**


# Refer to the following diagrams and let’s understand IPv4 Address

**Representation**



# Refer to the following case-study and let’s understand IPv4 Address

**Structure.**




In this scenario, representing a small office network, each network running on TCP must have a unique number, and every machine on it must have a unique IP address.


An IPv4 address is a 32-bit hierarchical address that is made up of a network portion and a host portion.

When determining the network portion versus the host portion, you must look at the 32-bit stream.

A subnet mask is used to determine the network and host portions.




## IPv4 Address Structure



**IPv4 Address Structure using Binary format**

# IPv4 Address Structure : Subnet Mask



To identify the network and host portions of an IPv4 address, the subnet mask is compared to the IPv4 address bit by bit, from left to right.


The actual process used to identify the network and host portions is called ANDing.

# IPv4 Address Structure: Prefix Length


A prefix length is a less cumbersome method used to identify a subnet mask address. The prefix length is the number of bits set to 1 in the subnet mask.

It is written in “slash notation” therefore, count the number of bits in the subnet mask and

prepend it with a slash.




# Types of IPv4 Addresses: Legacy Classful Addressing




Classful addressing wasted many IPv4 addresses.


Classful address allocation was replaced with classless addressing which ignores the rules of classes (A, B, C).



**Exercise-1**(Note: Start allocation IP address number from PC0)



Redraw above diagram which includes IP address and MAC address. Take IP address and MAC address as per your knowledge. Insert image below.



* Ipconfig: fill table ipconfig of all computers PC0

|  |  |
| --- | --- |
| **Parameter** | **Value** |
| Link local IPV6 Address | FE80::20C:CFFF:FEA2:B975 |
| IP address | 192.168.0.1 |
| Subnet Mask | 255.255.255.0 |
| Default Gateway | 0.0.0.0 |
|  |  |

PC1

|  |  |
| --- | --- |
| **Parameter** | **Value** |
| Link local IPV6 Address | FE80::260:47FF:FE9D:9B9E |

|  |  |
| --- | --- |
| IP address | 192.168.0.2 |
| Subnet Mask | 255.255.255.0 |
| Default Gateway | 0.0.0.0 |
|  |  |

* Ipconfig /all: apply command on command prompt and write parameters and values in the following table.

PC0

|  |  |
| --- | --- |
| **Parameter** | **Value** |
| Physical Address | 000C.CFA2.B975 |
| Link local IPV6 Address | FE80::20C:CFFF:FEA2:B975 |
| IPv4 Address | 192.168.0.1 |
| Subnet Mask | 255.255.255.0 |
| Default Gateway | 0.0.0.0 |
| DHCPv6 Client DUID | 00-01-00-01-85-63-CB-5E-00-0C-CF-A2-B9-  75 |

PC1

|  |  |
| --- | --- |
| **Parameter** | **Value** |
| Physical Address | 0060.479D.9B9E |
| Link local IPV6 Address | FE80::20C:CFFF:FEA2:B975 |
| IPv4 Address | 192.168.0.2 |
| Subnet Mask | 255.255.255.0 |
| Default Gateway | 192.168.0.1 |
| DHCPv6 Client DUID | 00-01-00-01-3C-BA-CC-6E-00-60-47-9D-9B-  9E |

* Arp –a: before ping, write output of command from PC0 and PC1 computers PC0


|  |  |
| --- | --- |
| **Parameter** | **Value** |
| Internet Address | 192.168.0.2 |
| Physical Address | 0060.479d.9b9e |

|  |  |
| --- | --- |
| Type | dynamic |

PC1

|  |  |
| --- | --- |
| **Parameter** | **Value** |
| Internet Address | 192.168.0.1 |
| Physical Address | 000c.cfa2.b975 |
| Type | dynamic |



* Ping from PC0 to PC1 and vice versa and insert snap of output here.




* Arp –a: after ping, insert snap (below) of output of command from all computers




* Netstat: insert snap of output of command from all computers\



**Exercise-2:** (Note: Start allocation IP address number from PC0)



Redraw above diagram which includes IP address and MAC address. Take IP address and MAC address as per your instruction. Insert image below.



* Ipconfig: fill table ipconfig of all computers PC0

|  |  |
| --- | --- |
| Link local IPV6 Address | FE80::2E0:8FFF:FE27:7503 |
| IP address | 121.127.0.1 |
| Subnet Mask | 255.0.0.0 |
| Default Gateway | 0.0.0.0 |

PC1

|  |  |
| --- | --- |
| Link local IPV6 Address | FE80::2E0:8FFF:FEAD:677E |
| IP address | 121.127.0.2 |
| Subnet Mask | 255.0.0.0 |
| Default Gateway | 121.127.0.1 |

PC2

|  |  |
| --- | --- |
| Link local IPV6 Address | FE80::201:97FF:FE1C:6785 |
| IP address | 121.127.0.3 |
| Subnet Mask | 255.0.0.0 |
| Default Gateway | 121.127.0.1 |

PC3

|  |  |
| --- | --- |
| Link local IPV6 Address | FE80::290:2BFF:FE9A:536A |
| IP address | 121.127.0.4 |
| Subnet Mask | 255.0.0.0 |
| Default Gateway | 121.127.0.1 |

* Ipconfig /all: apply command on command prompt and write parameters and values in following table.

PC0

|  |  |
| --- | --- |
| **Parameter** | **Value** |
| Physical Address | 00E0.8F27.7503 |
| Link local IPV6 Address | FE80::2E0:8FFF:FE27:7503 |
| IPv4 Address | 121.127.0.1 |
| Subnet Mask | 255.0.0.0 |

|  |  |
| --- | --- |
| Default Gateway | 0.0.0.0 |
| DHCPv6 Client DUID | 00-01-00-01-6D-A1-14-85-00-E0-8F-  27-75-03 |

PC1

|  |  |
| --- | --- |
| **Parameter** | **Value** |
| Physical Address | 00E0.8FAD.677E |
| Link local IPV6 Address | FE80::2E0:8FFF:FEAD:677E |
| IPv4 Address | 121.127.0.2 |
| Subnet Mask | 255.0.0.0 |
| Default Gateway | 121.127.1 |
| DHCPv6 Client DUID | 00-01-00-01-04-74-AE-8B-00-E0-8F- AD-67-7E |

PC2

|  |  |
| --- | --- |
| **Parameter** | **Value** |
| Physical Address | 0001.971C.6785 |
| Link local IPV6 Address | FE80::201:97FF:FE1C:6785 |
| IPv4 Address | 121.127.0.3 |
| Subnet Mask | 255.0.0.0 |
| Default Gateway | 121.127.1 |
| DHCPv6 Client DUID | 00-01-00-01-80-3C-10-D3-00-01-97-  1C-67-85 |


PC3


|  |  |
| --- | --- |
| **Parameter** | **Value** |
| Physical Address | 0090.2B9A.536A |
| Link local IPV6 Address | FE80::290:2BFF:FE9A:536A |
| IPv4 Address | 121.127.0.4 |
| Subnet Mask | 255.0.0.0 |
| Default Gateway | 121.127.1 |
| DHCPv6 Client DUID | 00-01-00-01-CA-70-49-9B-00-90-2B-  9A-53-6A |

* Arp –a: before ping write/snap of output of command from all computers




* Ping from PC0 to PC1 and vice versa and get the output here.






* Arp –a: after ping write/snap of output of command from all computers




* Netstat: write/snap of output of command from all computers



**Exercise-3** (Note: Start allocation IP address number from PC0)



Redraw above diagram which includes IP address and MAC address. Take IP address and MAC address as per your instruction. Insert image below.



* Ipconfig: fill following table with output of ipconfig of computer.

PC0

|  |  |
| --- | --- |
| Link local IPV6 Address | FE80::201:64FF:FEB0:CA4B |
| IP address | 192.168.1.20 |
| Subnet Mask | 255.255.255.0 |
| Default Gateway | 192.168.1.100 |

PC1

|  |  |
| --- | --- |
| Link local IPV6 Address | FE80::20A:41FF:FE0B:2C65 |
| IP address | 192.168.2.10 |
| Subnet Mask | 255.255.255.0 |
| Default Gateway | 192.168.2.100 |

* Ipconfig /all: apply command on command prompt and write parameters and values in following table

PC0

|  |  |
| --- | --- |
| **Parameter** | **Value** |
| Physical Address | 0001.64B0.CA4B |
| Link local IPV6 Address | FE80::201:64FF:FEB0:CA4B |
| IPv4 Address | 192.168.1.20 |
| Subnet Mask | 255.255.255.0 |
| Default Gateway | 192.168.1.100 |
| DHCPv6 Client DUID | 00-01-00-01-19-6B-BD-5D-00-01-64-B0-CA-  4B |


PC1


|  |  |
| --- | --- |
| **Parameter** | **Value** |
| Physical Address | 000A.410B.2C65 |
| Link local IPV6 Address | FE80::20A:41FF:FE0B:2C65 |
| IP address | 192.168.2.10 |
| Subnet Mask | 255.255.255.0 |
| Default Gateway | 192.168.2.100 |
| DHCPv6 Client DUID | 00-01-00-01-B8-C9-CA-55-00-0A-41-0B-2C-  65 |

* Arp –a: before ping write/snap of output of command from all computers





* Ping from PC0 to PC1 and vice versa and get the output here.






* Arp –a: after ping write/snap of output of command from all computers



* Netstat: write/snap of output of command from all computers



Write answers to the following questions.

* 1. What are the conclusions of the ipconfig command?

Ans: Provides basic network configuration information such as IP address, subnet mask, and default gateway.

* 1. What are the conclusions of **ipconfig /all** commands?

Ans: Provides detailed network configuration information including IP address, subnet mask, default gateway, DNS server, MAC address, DHCP server, and more.

* 1. What are the conclusions of **arp -a** command before ping?

Ans:Displays the current ARP cache which maps IP addresses to MAC addresses for devices the computer has recently communicated with.

* 1. What are the conclusions of **netstat** -r command after ping?

Ans: Displays the routing table which shows the routes packets will take when traveling to specific IP addresses after performing a ping.

* 1. What is my MAC address?

Ans: Your MAC address is a unique identifier assigned to your network interface card (NIC). You can find it using **ipconfig /all** or **ifconfig** command on Windows or Linux respectively.

* 1. Which network is configured? Static and Dynamic

Ans: Static: Network configuration where IP address, subnet mask, gateway, etc., are manually set.

Dynamic: Network configuration where IP address and other network parameters are automatically assigned by a DHCP server.

* 1. What is my gateway?

Ans: Your gateway is the IP address of the device that serves as the access point to other networks, typically your router.

* 1. What is a hostname?

Ans: :A hostname is a label assigned to a device connected to a computer network. It's used to identify the device within the network.

* 1. What is my IPv6 address?

Ans:Your IPv6 address is a unique identifier assigned to your device on an IPv6 network. You can find it using **ipconfig /all** or **ifconfig** command.

* 1. What is ARPA?

Ans:ARPA stands for Address and Routing Parameter Area. It's a top-level domain used in the reverse DNS lookup to map IP addresses to domain names.

* 1. What is a loopback address?

Ans:The loopback address (127.0.0.1 for IPv4 and ::1 for IPv6) is a special address assigned to the local machine, allowing it to send data to itself.

* 1. What does Port 80 mean?

Ans: Port 80 is the default port for Hypertext Transfer Protocol (HTTP), the protocol used for transmitting web pages over the internet.

* 1. What is the difference between logical address and physical address?
* Ans: Logical Address: Used at the network layer to uniquely identify a device on a network, e.g., IP address.
* Physical Address: Also known as MAC address, it's a hardware address assigned to the network interface card (NIC) and used at the data link layer to uniquely identify a device on a network.
  1. What is NetBIOS?

Ans: NetBIOS (Network Basic Input/Output System) is a networking protocol used for communication between devices on a local network, often used in Windows environments

# Gate Questions :

## Traceroute reports a possible route that is taken by packets moving from some host A to some other host B. Which of the following options represents the technique used by traceroute to identify these hosts:

* 1. By progressively querying routers about the next router on the path to B using ICMP packets, starting with the first router
  2. By requiring each router to append the address to the ICMP packet as it is forwarded to B. The list of all routers en-route to B is returned by B in an ICMP reply packet
  3. By ensuring that an ICMP reply packet is returned to A by each router en-route to B, in the ascending order of their hop distance from A
  4. By locally computing the shortest path from A to B

## Which of the following assertions is FALSE about the Internet Protocol (IP)?

* 1. It is possible for a computer to have multiple IP addresses
  2. IP packets from the same source to the same destination can take different routes in the network
  3. IP ensures that a packet is discarded if it is unable to reach its destination within a given number of hops
  4. The packet source cannot set the route of an outgoing packets; the route is determined only by the routing tables in the routers on the way

## Consider three IP networks A, B and C. Host HA in network A sends messages each containing 180 bytes of application data to a host HC in network C. The TCP layer prefixes 20 byte header to the message.

**This passes through an intermediate network B.The maximum packet size, including 20 byte IP header, in each network is:**

## A: 1000 bytes

**B: 100 bytes**

## C: 1000 bytes

**The network A and B are connected through a 1 Mbps link, while B and C are connected by a 512 Kbps link (bps = bits per second).**

## Assuming that the packets are correctly delivered, how many bytes, including headers, are delivered to the IP layer at the destination for one application message, in the best case? Consider only data packets.

A) 200

B) 220

C) 240

D) 260

## Consider three IP networks A, B and C. Host HA in network A sends messages each containing 180 bytes of application data to a host HC in network C. The TCP layer prefixes 20 byte header to the message. This passes through an intermediate network

**B. The maximum packet size, including 20 byte IP header, in each network, is: A : 1000 bytes**

## B : 100 bytes C : 1000 bytes

**The network A and B are connected through a 1 Mbps link, while B and C are connected by a 512 Kbps link (bps = bits per second).**

## I.

**What is the rate at which application data is transferred to host HC? Ignore errors,**

## acknowledgments, and other overheads.

1. 325.5 Kbps
2. 354.5 Kbps
3. 409.6 Kbps D) 512.0 Kbps

## In the IPv4 addressing format, the number of networks allowed under Class C addresses is:

A) 214

B) 227

C) 221

D) 224

## Correct options. need to be changed.

1. **In an IPv4 datagram, the M bit is 0, the value of HLEN is 10, the value of total length is 400 and the fragment offset value is 300. The position of the datagram, the sequence numbers of the first and the last bytes of the payload, respectively are:**
   1. Last fragment, 2400 and 2789
   2. First fragment, 2400 and 2759 C) Last fragment, 2400 and 2759

D) Middle fragment, 300 and 689

## There are n stations in slotted LAN. Each station attempts to transmit with a probability p in each time slot. What is the probability that ONLY one station transmits in a given time slot?

* 1. np(1 − p)n−1 B) (1 − p)n−1

C) p(1 − p)n−1

D) 1 − (1 − p)n−1

## The subnet mask for a particular network is 255.255.31.0. Which of the following pairs of IP addresses could belong to this network?

A) 172.57.88.62 and 172.56.87.23

B) 10.35.28.2 and 10.35.29.4

C) 191.203.31.87 and 191.234.31.88

D) 128.8.129.43 and 128.8.161.55

## The routing table of a router is shown below:

|  |  |  |
| --- | --- | --- |
| **Destination** | **Subnet Mask** | **Interface** |
| **128.75.43.0** | **255.255.255.0** | **Eth0** |
| **128.75.43.0** | **255.255.255.128** | **Eth1** |
| **192.12.17.5** | **255.255.255.255** | **Eth3** |
| **Default** |  | **Eth2** |

**On which interface will the router forward packets addressed to destinations 128.75.43.16 and 192.12.17.10 respectively?**

* 1. Eth1 and Eth2
  2. Eth0 and Eth2
  3. Eth0 and Eth3
  4. Eth1 and Eth3

## An organization has a class B network and wishes to form subnets for 64 departments. The subnet mask would be:

A) 255.255.0.0

B) 255.255.64.0

C) 255.255.128.0

D) 255.255.252.0

## Two computers C1 and C2 are configured as follows. C1 has IP address 203.197.2.53 and netmask 255.255.128.0 .C2 has IP address 203.197.75.201 and netmask 255.255.192.0 . Which one of the following statements is true?

* 1. C1 and C2 both assume they are on the same network
  2. C2 assumes C1 is on same network, but C1 assumes C2 is on a different network
  3. C1 assumes C2 is on same network, but C2 assumes C1 is on a different network
  4. C1 and C2 both assume they are on different networks.

## The address of a class B host is to be split into subnets with a 6-bit subnet number. What is the maximum number of subnets and the maximum number of hosts in each subnet?

* 1. 62 subnets and 262142 hosts.
  2. 64 subnets and 262142 hosts.
  3. 62 subnets and 1022 hosts.
  4. 64 subnets and 1024 hosts.

## If a class B network on the Internet has a subnet mask of 255.255.248.0 , what is the maximum number of hosts per subnet?

A) 1022

B) 1023

C) 2046

D) 2047

## Suppose computers A and B have IP addresses 10.105.1.113 and 10.105.1.91 respectively and they both use same netmask N. Which of the values of N given below should not be used if A and B should belong to the same network?

A) 255.255.255.0

B) 255.255.255.128

C) 255.255.255.192

D) 255.255.255.224

## An Internet Service Provider (ISP) has the following chunk of CIDR-based IP addresses available with it: 245.248.128.0/20 . The ISP wants to give half of this chunk of addresses to Organization A, and a quarter to Organization B, while retaining the remaining with itself. Which of the following is a valid allocation of addresses to A and B?

A) 245.248.136.0/21 and 245.248.128.0/22

B) 245.248.128.0/21 and 245.248.128.0/22

C) 245.248.132.0/22 and 245.248.132.0/21

D) 245.248.136.0/24 and 245.248.132.0/21

## Consider the following routing table at an IP router:

|  |  |  |
| --- | --- | --- |
| **Network No** | **Net Mask** | **Next Hop** |
| **128.96.170.**  **0** | **255.255.254.0** | **Interface 0** |
| **128.96.168.**  **0** | **255.255.254.0** | **Interface 1** |
| **128.96.166.**  **0** | **255.255.254.0** | **R2** |
| **128.96.164.**  **0** | **255.255.252.0** | **R3** |
| **0.0.0.0** | **Default** | **R4** |

**For each IP address in Group I Identify the correct choice of the next hop from Group II using the entries from the routing table above.**

|  |  |
| --- | --- |
| **Group I** | **Group II** |
| **i) 128.96.171.92** | **a) Interface 0** |
| **ii) 128.96.167.151** | **b) Interface 1** |
| **iii) 128.96.163.151** | **c) R2** |
| **iv) 128.96.164.121** | **d) R3** |
|  | **e) R4** |

* 1. i-a, ii-c, iii-e, iv-d
  2. i-a, ii-d, iii-b, iv-e
  3. i-b, ii-c, iii-d, iv-e
  4. i-b, ii-c, iii-e, iv-d

## In the network 200.10.11.144/27 , the fourth octet (in decimal) of the last IP address of the network which can be assigned to a host is .

1. **Consider three machines M, N, and P with IP addresses 100.10.5.2, 100.10.5.5 , and**

## 100.10.5.6 respectively. The subnet mask is set to 255.255.255.252 for all the three machines. Which one of the following is true?

1. M, N, and P all belong to the same subnet
2. Only M and N belong to the same subnet
3. Only N and P belong to the same subnet
4. M, N, and P belong to three different subnets

## An organization requires a range of IP address to assign one to each of its 1500 computers. The organization has approached an Internet Service Provider (ISP) for this task. The ISP uses CIDR and serves the requests from the available IP address space 202.61.0.0/17 . The ISP wants to assign an address space to the organization which will minimize the number of routing entries in the ISP’s router using route aggregation. Which of the following address spaces are potential candidates from which the ISP can allot any one of the organization?

**I. 202.61.84.0/21**

## II. 202.61.104.0/21

**III. 202.61.64.0/21**

## IV. 202.61.144.0/21

* 1. I and II only
  2. II and III only
  3. III and IV only
  4. I and IV only

## A subnet has been assigned a subnet mask of 255.255.255.192 . What is the maximum number of hosts that can belong to this subnet?

* 1. 14
  2. 30
  3. 62

D) 126

## A company has a class C network address of 204.204.204.0 . It wishes to have three subnets, one with 100 hosts and two with 50 hosts each. Which one of the following options represents a feasible set of subnet address/subnet mask pairs?

A) 204.204.204.128/255.255.255.192 204.204.204.0/255.255.255.128

204.204.204.64/255.255.255.128

B) 204.204.204.0/255.255.255.192 204.204.204.192/255.255.255.128

204.204.204.64/255.255.255.128

C) 204.204.204.128/255.255.255.128 204.204.204.192/255.255.255.192

204.204.204.224/255.255.255.192

D) 204.204.204.128/255.255.255.128 204.204.204.64/255.255.255.192

204.204.204.0/255.255.255.192

## A subnetted Class B network has the following broadcast address: 144.16.95.255. Its subnet mask

* 1. is necessarily 255.255.224.0
  2. is necessarily 255.255.240.0
  3. is necessarily 255.255.248.0

D) could be any one of 255.255.224.0 , 255.255.240.0 ,255.255.248.0

## Host X has IP address 192.168.1.97 and is connected through two routers R1 and R2 to another host Y with IP address 192.168.1.80. Router R1 has IP addresses 192.168.1.135 and 192.168.1.110 . R2 has IP addresses 192.168.1.67 and 192.168.1.155 . The netmask used in the network is 255.255.255.224 .

1. **Given the information above, how many distinct subnets are guaranteed to already exist in the network?**
   1. 1
   2. 2
   3. 3
   4. 6

## Host X has IP address 192.168.1.97 and is connected through two routers R1 and R2 to another host Y with IP address 192.168.1.80. Router R1 has IP addresses 192.168.1.135 and 192.168.1.110 . R2 has IP addresses 192.168.1.67 and 192.168.1.155 . The netmask used in the network is 255.255.255.224 .

1. **Which IP address should X configure its gateway as?**

A) 192.168.1.67

B) 192.168.1.110

C) 192.168.1.135

D) 192.168.1.155

## A computer on a 10 Mbps network is regulated by a token bucket. The token bucket is filled at a rate of 2 Mbps. It is initially filled to capacity with 16 Megabits. What is the maximum duration for which the computer can transmit at the full 10 Mbps?

* 1. 1.6 seconds
  2. 2 seconds
  3. 5 seconds
  4. 8 seconds

## For a host machine that uses the token bucket algorithm for congestion control, the token bucket has a capacity of 1 megabyte and the maximum output rate is 20 megabytes per second. Tokens arrive at a rate to sustain output at a rate of 10 megabytes per second. The token bucket is currently full and the machine needs to send

**12 megabytes of data. The minimum time required to transmit the data is seconds.**

## In the diagram shown below, L1 is an Ethernet LAN and L2 is a Token-Ring LAN. An IP packet originates from sender S and traverses to R, as shown. The links within each ISP and across the two ISPs, are all point-to-point optical links. The initial value of the TTL field is 32. The maximum possible value of the TTL field when R receives the datagram is .

